% MARVIN NLL register values generated on 05-Aug-2020 with the Noise Calibration Tool v1.00

% First image of the high-light capture series: F:\file\tuning\20202803\IMX485_12bit_bggr_25601440\NR\high_light\P0731143723.raw

% First image of the low-light capture series: F:\file\tuning\20202803\IMX485_12bit_bggr_25601440\NR\low_light\P0731144156.raw

NLL_SEGMENTATION = 1   % 1: logarithmic knot distribution

nll_coeff_n = [4095  4095  4095  4095  2588  1528  1189  1007   889   741   648   583   497   440   399   368   343];

%0xFFF 0xFFF 0xFFF 0xFFF 0xA1C 0x5F8 0x4A5 0x3EF 0x379 0x2E5 0x288 0x247 0x1F1 0x1B8 0x18F 0x170 0x157 