% MARVIN NLL register values generated on 28-Jul-2011 with the Noise Calibration Tool v1.00

% First image of the high-light capture series: \\dctfiler1\home\neugebauer\CHARACTERIZATION\OV14825_MIPI\01_exGoldenSample\Noise\1920x1080\Gain001\Overexposure\mrv_030_001_1311607836757218_0000.pgm

% First image of the low-light capture series: \\dctfiler1\home\neugebauer\CHARACTERIZATION\OV14825_MIPI\01_exGoldenSample\Noise\1920x1080\Gain001\Underexposure\mrv_030_001_1311608768132563_0000.pgm

NLL_SEGMENTATION = 1;   % 1: logarithmic knot distribution

nll_coeff_n = [4095  3437  2358  1907  1643  1335  1154  1031   940   813   727   663   574   513   468   434   406];

%0xFFF 0xD6D 0x936 0x773 0x66B 0x537 0x482 0x407 0x3AC 0x32D 0x2D7 0x297 0x23E 0x201 0x1D4 0x1B2 0x196 